_________________

Entity

PLAYGROUND SAFETY CHECKLIST

Monthly Inspection

Park/Playground Name: _____________________
Inspector’s Name: ____________________

Address: _________________________________
Date: _______________________________

                                 



       Yes     No     N/A                       Comments

	General Area
	
	
	
	

	1. Is the play area and access free of poor drainage, exposed pipes, and slipping and tripping hazards such as ice, tree roots and leaves, irrigation heads, etc.?
	
	
	
	

	2.  Is adequate lighting provided?  When was it last checked at night?
	
	
	
	

	3.  Are restrooms and water fountains clean and functioning properly?
	
	
	
	

	4.  If sand or gravel is used as the protective surface, is it raked regularly, rototilled annually and of sufficient depth in all areas?
	
	
	
	

	5.  Are all footings covered with the proper depth of protective surfacing?
	
	
	
	

	6.  Is the protective surfacing free of debris, animal feces, rocks, glass or other foreign objects?
	
	
	
	

	7.  Is the play area closed if the protective surfacing is frozen?
	
	
	
	

	8.  Is the perimeter environment such as benches and tables, etc. in good repair?
	
	
	
	

	9.  Are all tree limbs trimmed to greater than 7 feet above the ground?
	
	
	
	

	10.  Are all wood items free of splinters?
	
	
	
	

	11.  Are all points, corners and edges of items free of sharp areas?  Are open ends of tubing sealed?
	
	
	
	

	
	
	
	
	

	Climbing Equipment
	
	
	
	

	12.  Are flexible grid climbing devices such as net and chain climbers, and tire climbers securely anchored at both ends?
	
	
	
	

	13.  Are connections between ropes, cables, chains or tires securely fixed?
	
	
	
	

	
	
	
	
	

	Climbing Ropes
	
	
	
	

	14.  Are ropes secured at both ends and not capable of creating a loop with an inside perimeter greater than 5 inches?


	
	
	
	

	
	Yes
	No
	N/A
	                  Comments

	Merry-Go-Rounds 
	
	
	
	

	15.  Is the underside of the platform no less than 9 inches above the protective surfacing?
	
	
	
	

	16.  Is the maximum height of the standing surface 14 inches above the protective surface?
	
	
	
	

	17.  Is the platform surface free of sharp edges and continuous with no openings between the axis and periphery 5/16 inch or greater?
	
	
	
	

	18.  Is the speed of rotation limited to a maximum of 13 feet per second?
	
	
	
	

	19.  Is the platform free of up and down motion?
	
	
	
	

	
	
	
	
	

	Slides
	
	
	
	

	20.  For slides no more than 4 feet in height, is the exit region no more than 11 inches from the protective surfacing? 
	
	
	
	

	21.  For slides over 4 feet in height, is the exit region at least 7 but not more than 15 inches above the protective surfacing?
	
	
	
	

	22.  For roller slides, are all rollers in place with no broken bearings?
	
	
	
	

	
	
	
	
	

	Swings
	
	
	
	

	23.  Are S-hooks pinched shut or closed with a gap no greater than 0.04 inch?  The gap should not admit a dime.
	
	
	
	

	24.  Is the vertical distance from the underside of an occupied swing seat to the protective surfacing no less than 12 inches for preschool age children and school age children?
	
	
	
	

	
	
	
	
	

	Tot Swings
	
	
	
	

	25.  Is the vertical distance from the underside of an occupied swing seat to the protective surfacing no less than 24 inches?
	
	
	
	

	
	
	
	
	

	Multi-Axis Tire Swings
	
	
	
	

	26.  If steel-belted radials are used, are the steel belts concealed?
	
	
	
	


Additional Comments

